SCBA/RIT Instructor Notes

SCBA/PPE donning

· Emphasize doing it correctly before quickly.
· Emphasize seated SCBA donning over other methods.
· Emphasize the need for buckling the waist belt, SCBA can be used for dragging a downed firefighter.
· Practice putting the mask on while using structural firefighting gloves.
· [bookmark: _GoBack]Steps for donning seated are included in this document to be used as a handout, if desired, or refer to full ‘Donning SCBA’ word document, beginning on page 3, for donning steps.
· Standard at end of the training is for the firefighter to be able to don the SCBA equipment and be ready to be ‘on air’ in 1 minute or less, while wearing full turnout gear.








Rit CPR

· Watch video prior to class, so you are familiar with the steps outlined in the power point.
· The steps in the video go by pretty fast, it may be beneficial to watch it more than once.
· Emphasize the importance of Rescuer 1’s job of securely holding the straps and coat when setting up for the pull down.
· Try to have at least one group demonstrate live. If time allows, have more do the drill, ideally as Rescuer 1 and 3 or 4.










Seated SCBA Donning

1. Procedure to don seat mounted SCBA
a) Open the cylinder valve fully
b) Check the cylinder and the remote gauge readings
(1) Pressure readings must be within 100 psi
(2) Needles on both gauges indicate the same pressure for gauges without 100 psi increments
c) Position your body in the seat with your back firmly against the SCBA and release the SCBA hold-down device
d) Insert your arms through the shoulder straps
e) Fasten the chest straps, buckle the waist strap, and adjust the shoulder straps
f) Fasten your seat belt before the apparatus moves
g) Don the facepiece and check the facepiece seal
h) Connect the air supply to the facepiece when you are ready to use it
a) Activate the PASS device manually if it is not integrated in the system (See Township Fire SOG 2-1-7 for specific alerts for this PASS device)
i) Don the hood, the helmet, and the gloves
2. Exit the fire apparatus carefully to avoid slips or falls due to the extra weight on your back


